,txt##OTHER##,Height##LENGTH##MILLIMETERS,Length##LENGTH##MILLIMETERS,Width##LENGTH##MILLIMETERS,Weight##MASS##KILOGRAMS,Voltage##ELECTRICAL_POTENTIAL##VOLTS,Frequency##ELECTRICAL_FREQUENCY##HERTZ,Cooling capacity##HVAC_COOLING_LOAD##KILOWATTS,Cooling Total Input Power##HVAC_POWER##KILOWATTS,Cooling Water Flow Rate##PIPING_FLOW##LITERS_PER_SECOND,Available Pressure (Cooling)##PIPING_PRESSURE##KILOPASCALS,Heating Capacity##HVAC_HEATING_LOAD##KILOWATTS,Heating Total Input Power##HVAC_POWER##KILOWATTS,Heating Water Flow Rate##PIPING_FLOW##LITERS_PER_SECOND,Available Pressure (Heating)##PIPING_PRESSURE##KILOPASCALS,Air Flow Rate##HVAC_AIR_FLOW##CUBIC_METERS_PER_HOUR,Sound Power Level##OTHER##,Sound Pressure Level##OTHER##,Logo visibility##OTHER##,Clearance Visibility##OTHER##,Hydronic Out Offset Left View##LENGTH##MILLIMETERS,Hydronic In Offset Left View##LENGTH##MILLIMETERS,Hydronic Out Offset Top View##LENGTH##MILLIMETERS,Hydronic In Offset Top View##LENGTH##MILLIMETERS,Hydraulic Connection Diameter OUT##PIPE_SIZE##INCHES,Hydraulic Connection Diameter IN##PIPE_SIZE##INCHES,Commenti sul tipo##OTHER##,URL##OTHER##,Modello##OTHER##,Total Input Current (Cooling)##ELECTRICAL_CURRENT##AMPERES,Total Input Current (Heating)##ELECTRICAL_CURRENT##AMPERES,Maximum Current (FLA)##ELECTRICAL_CURRENT##AMPERES,Starting Current (LRA)##ELECTRICAL_CURRENT##AMPERES,Manufacturer Telefax##OTHER##,Manufacturer Phone##OTHER##,Manufacturer Country##OTHER##,Manufacturer Address##OTHER##,Produttore##OTHER##,Descrizione##OTHER##,Data Sheet##OTHER##,Costo##CURRENCY##,Copyright##OTHER##,Coat Material##OTHER##
ANKI-HX_20,AERMEC - ANKI HX,1028,1000,346,82,230,50,6,1.89,0.285,74,6.08,1.86,0.295,76,3590,64.0dB(A),32.7dB(A),1,1,369,134,57,76.5,1,1,Heat Pumps,http://global.aermec.com/en,ANKI - HX,9,11.2,12.9,8.8,+39 0442 93577,+39 0442 633111,Italy,Via Roma _996 _37040_Bevilacqua_(VR),AERMEC S.P.A.,Reversible inverter heat pump Air/Water outdoor installation,http://download.aermec.com/docs/schede/anki_1603_en.pdf?r=6844,0,Copyright_AERMEC,Aermec_Ral9002
ANKI-HX_25,AERMEC - ANKI HX,1028,1000,346,82,230,50,7.49,2.52,0.349,68,7.61,2.36,0.375,69,3590,65.4dB(A),34.1dB(A),1,1,369,134,57,76.5,1,1,Heat Pumps,http://global.aermec.com/en,ANKI - HX,11.8,13.9,14.9,8.8,+39 0442 93577,+39 0442 633111,Italy,Via Roma _996 _37040_Bevilacqua_(VR),AERMEC S.P.A.,Reversible inverter heat pump Air/Water outdoor installation,http://download.aermec.com/docs/schede/anki_1603_en.pdf?r=6844,0,Copyright_AERMEC,Aermec_Ral9002
