,txt##OTHER##,Height##LENGTH##MILLIMETERS,Length##LENGTH##MILLIMETERS,Width##LENGTH##MILLIMETERS,Weight##MASS##KILOGRAMS,Voltage##ELECTRICAL_POTENTIAL##VOLTS,Number of Poles##OTHER##,Frequency##ELECTRICAL_FREQUENCY##HERTZ,Cooling capacity##HVAC_COOLING_LOAD##KILOWATTS,Cooling Total Input Power##HVAC_POWER##KILOWATTS,Cooling Water Flow Rate##PIPING_FLOW##LITERS_PER_SECOND,Available Pressure (Cooling)##PIPING_PRESSURE##KILOPASCALS,Heating Capacity##HVAC_HEATING_LOAD##KILOWATTS,Heating Total Input Power##HVAC_POWER##KILOWATTS,Heating Water Flow Rate##PIPING_FLOW##LITERS_PER_SECOND,Available Pressure (Heating)##PIPING_PRESSURE##KILOPASCALS,Air Flow Rate##HVAC_AIR_FLOW##CUBIC_METERS_PER_HOUR,Sound Power Level##OTHER##,Sound Pressure Level##OTHER##,Logo visibility##OTHER##,Clearance Visibility##OTHER##,Hydronic Out Offset Left View##LENGTH##MILLIMETERS,Hydronic In Offset Left View##LENGTH##MILLIMETERS,Hydronic Out Offset Top View##LENGTH##MILLIMETERS,Hydronic In Offset Top View##LENGTH##MILLIMETERS,Hydraulic Connection Diameter OUT##PIPE_SIZE##INCHES,Hydraulic Connection Diameter IN##PIPE_SIZE##INCHES,Commenti sul tipo##OTHER##,URL##OTHER##,Modello##OTHER##,Total Input Current (Cooling)##ELECTRICAL_CURRENT##AMPERES,Total Input Current (Heating)##ELECTRICAL_CURRENT##AMPERES,Maximum Current (FLA)##ELECTRICAL_CURRENT##AMPERES,Starting Current (LRA)##ELECTRICAL_CURRENT##AMPERES,Manufacturer Telefax##OTHER##,Manufacturer Phone##OTHER##,Manufacturer Country##OTHER##,Manufacturer Address##OTHER##,Produttore##OTHER##,Descrizione##OTHER##,Data Sheet##OTHER##,Costo##CURRENCY##,Copyright##OTHER##,Coat Material##OTHER##
ANK-HA_20,AERMEC - ANK HA,1028,1358,400,160,400,3,50,6.84,2.41,0.326,65,7.867,2.56,0.380,62,3500,68dB(A),37dB(A),1,1,205,110,297,411,1.25,1.25,Heat Pumps,http://global.aermec.com/en,ANK - HA,4.3,4.7,6.1,39.7,+39 0442 93577,+39 0442 633111,Italy,Via Roma _996 _37040_Bevilacqua_(VR),AERMEC S.P.A., Reversible heat pumps Air/Water for external installation,http://download.aermec.com/docs/schede/ank_en.pdf?r=6856,0,Copyright_AERMEC,Aermec_Ral9002
